
**** 10/16/05 19:38:04 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Fully CMOS\Schematic1.sch


 ****     CIRCUIT DESCRIPTION


******************************************************************************




* Schematics Version 9.2
* Sun Oct 16 19:38:03 2005



** Analysis setup **
.tran 1n 2u 0 200p
.STMLIB "Schematic1.stl"


* From [PSPICE NETLIST] section of C:\Program Files\Orcad\PSpice\PSpice.ini:
.lib "nom.lib"

.INC "Schematic1.net"



**** INCLUDING Schematic1.net ****
* Schematics Netlist *



M_M1         inv_out a 0 0 MbreakN           
M_M2         Vdd a inv_out Vdd MbreakP           
M_M4         $N_0002 b $N_0001 0 MbreakN           
M_M3         nand_out a $N_0002 0 MbreakN           
M_M7         nor_out a $N_0003 0 MbreakN           
M_M8         nor_out b $N_0003 0 MbreakN           
M_M11         $N_0001 clk 0 0 MbreakN           
M_M12         $N_0003 clk 0 0 MbreakN           
M_M14         Vdd clk nor_out Vdd MbreakP           
M_M13         Vdd clk nand_out Vdd MbreakP           
V_V1         Vdd 0 DC 5 AC 0 
V_V3         b 0   STIMULUS=V3
V_V2         a 0   STIMULUS=V2
V_V4         clk 0   STIMULUS=V4

**** RESUMING Schematic1.cir ****
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 


.END

* C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Fully CMOS\Schematic1.stl written on Sun 
* by Stimulus Editor -- Serial Number: 1 -- Version 9.2
;!Stimulus Get
;! V2 Analog V3 Analog V4 Analog
;!Ok
;!Plot Axis_Settings
;!Xrange 0s 6us
;!Yrange 0 5
;!AutoUniverse
;!XminRes 1ns
;!YminRes 1n
;!Ok
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )
.STIMULUS V3 PULSE( 0 5 0 10p 10p 1u 2u )
.STIMULUS V4 PULSE( 0 5 0 1p 1p 100n 200n )
.STIMULUS V3 PULSE( 0 5 0 10p 10p 1u 2u )
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )

**** 10/16/05 19:38:04 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Fully CMOS\Schematic1.sch


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               MbreakN         MbreakP         
               NMOS            PMOS            
       LEVEL    1               1            
           L  100.000000E-06  100.000000E-06 
           W  100.000000E-06  100.000000E-06 
         VTO    0               0            
          KP   20.000000E-06   20.000000E-06 
       GAMMA    0               0            
         PHI     .6              .6          
      LAMBDA    0               0            
          IS   10.000000E-15   10.000000E-15 
          JS    0               0            
          PB     .8              .8          
        PBSW     .8              .8          
          CJ    0               0            
        CJSW    0               0            
        CGSO    0               0            
        CGDO    0               0            
        CGBO    0               0            
         TOX    0               0            
          XJ    0               0            
       UCRIT   10.000000E+03   10.000000E+03 
      DIOMOD    1               1            
         VFB    0               0            
        LETA    0               0            
        WETA    0               0            
          U0    0               0            
        TEMP    0               0            
         VDD    0               0            
       XPART    0               0            


**** 10/16/05 19:38:04 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Fully CMOS\Schematic1.sch


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    0.0000  (    b)    0.0000  (  clk)    0.0000  (  Vdd)    5.0000      

($N_0001)-482.2E-09                   ($N_0002)-482.2E-09                       

($N_0003)-543.6E-09                   (inv_out)    5.0000                       

(nor_out)    5.0000                   (nand_out)    5.0000                  




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -2.004E-11
    V_V3         0.000E+00
    V_V2         0.000E+00
    V_V4         0.000E+00

    TOTAL POWER DISSIPATION   1.00E-10  WATTS


ERROR -- Convergence problem in transient analysis at Time =  1.100E-06
         Time step =  762.9E-21, minimum allowable step size =  2.000E-18

  These voltages failed to converge:

    V($N_0002)                =     4.992V  \     4.984V

  These devices failed to converge:
    M_M3      

ERROR -- Discontinuing simulation due to convergence problem


  Last node voltages tried were:

 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    5.0000  (    b)    0.0000  (  clk)    4.9988  (  Vdd)    5.0000      

($N_0001)-23.05E-24                   ($N_0002)    4.9921                       

($N_0003) 204.1E-09                   (inv_out) 50.10E-09                       

(nor_out) 408.1E-09                   (nand_out)    4.9990                  


 **** Runtime Parameters
                              
      ABSTOL =      1.0000E-12
        GMIN =      1.0000E-12
        ITL1 =      1.5000E+02
        ITL2 =      2.0000E+01
        ITL4 =      1.0000E+01
      RELTOL =      1.0000E-03
      RUNFOR =      0.0000E+00
        TMAX =      2.0000E-10
       TSTOP =      2.0000E-06
       VNTOL =      1.0000E-06
              
               

ERROR -- Convergence problem in transient analysis at Time =  1.100E-06
         Time step =  762.9E-21, minimum allowable step size =  2.000E-18

  These voltages failed to converge:

    V($N_0002)                =     4.992V  \     4.984V

  These devices failed to converge:
    M_M3      

ERROR -- Discontinuing simulation due to convergence problem


  Last node voltages tried were:

 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    5.0000  (    b)    0.0000  (  clk)    4.9988  (  Vdd)    5.0000      

($N_0001)-23.05E-24                   ($N_0002)    4.9921                       

($N_0003) 204.1E-09                   (inv_out) 50.10E-09                       

(nor_out) 408.1E-09                   (nand_out)    4.9990                  


 **** Runtime Parameters
                              
      ABSTOL =      1.0000E-12
        GMIN =      1.0000E-12
        ITL1 =      1.5000E+02
        ITL2 =      2.0000E+01
        ITL4 =      1.0000E+01
      RELTOL =      1.0000E-03
      RUNFOR =      0.0000E+00
        TMAX =      2.0000E-10
       TSTOP =      2.0000E-06
       VNTOL =      1.0000E-06
              
               

ERROR -- Convergence problem in transient analysis at Time =  1.100E-06
         Time step =  762.9E-21, minimum allowable step size =  2.000E-18

  These voltages failed to converge:

    V($N_0002)                =     4.992V  \     4.984V

  These devices failed to converge:
    M_M3      

ERROR -- Discontinuing simulation due to convergence problem


  Last node voltages tried were:

 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    5.0000  (    b)    0.0000  (  clk)    4.9988  (  Vdd)    5.0000      

($N_0001)-23.05E-24                   ($N_0002)    4.9921                       

($N_0003) 204.1E-09                   (inv_out) 50.10E-09                       

(nor_out) 408.1E-09                   (nand_out)    4.9990                  

