
**** 03/07/06 20:23:54 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Pass Transistor\Schematic1.sch


 ****     CIRCUIT DESCRIPTION


******************************************************************************




* Schematics Version 9.2
* Tue Mar 07 20:23:51 2006



** Analysis setup **
.tran 1n 2u 0 200p
.STMLIB "Schematic1.stl"


* From [PSPICE NETLIST] section of C:\Program Files\Orcad\PSpice\PSpice.ini:
.lib "nom.lib"

.INC "Schematic1.net"



**** INCLUDING Schematic1.net ****
* Schematics Netlist *



V_V1         Vdd 0 DC 5 AC 0 
V_V2         a 0   STIMULUS=V2
V_V3         b 0   STIMULUS=V3
M_M12         Vdd $N_0001 nand_out Vdd MbreakP           
M_M11         nand_out $N_0001 0 0 MbreakN           
M_M16         a $N_0002 $N_0001 Vdd MbreakP           
M_M15         $N_0001 b a 0 MbreakN           
M_M21         Vdd $N_0003 nor_out Vdd MbreakP           
M_M22         nor_out $N_0003 0 0 MbreakN           
M_M23         a b $N_0003 Vdd MbreakP           
M_M27         $N_0003 b b 0 MbreakN           
M_M28         b $N_0004 $N_0003 Vdd MbreakP           
M_M24         Vdd b $N_0004 Vdd MbreakP           
M_M25         $N_0004 b 0 0 MbreakN           
M_M26         $N_0003 $N_0004 a 0 MbreakN           
M_M1         inv_out a 0 0 MbreakN           
M_M2         Vdd a inv_out Vdd MbreakP           
M_M20         $N_0002 b 0 0 MbreakN           
M_M19         Vdd b $N_0002 Vdd MbreakP           
M_M18         $N_0001 $N_0002 b 0 MbreakN           
M_M17         b b $N_0001 Vdd MbreakP           

**** RESUMING Schematic1.cir ****
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 


.END

* C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Pass Transistor\Schematic1.stl written on
* by Stimulus Editor -- Serial Number: 1 -- Version 9.2
;!Stimulus Get
;! V2 Analog V3 Analog
;!Ok
;!Plot Axis_Settings
;!Xrange 0s 6us
;!Yrange 0 5
;!AutoUniverse
;!XminRes 1ns
;!YminRes 1n
;!Ok
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )
.STIMULUS V3 PULSE( 0 5 0 10p 10p 1u 2u )
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )

**** 03/07/06 20:23:54 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Pass Transistor\Schematic1.sch


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               MbreakP         MbreakN         
               PMOS            NMOS            
       LEVEL    1               1            
           L  100.000000E-06  100.000000E-06 
           W  100.000000E-06  100.000000E-06 
         VTO    0               0            
          KP   20.000000E-06   20.000000E-06 
       GAMMA    0               0            
         PHI     .6              .6          
      LAMBDA    0               0            
          IS   10.000000E-15   10.000000E-15 
          JS    0               0            
          PB     .8              .8          
        PBSW     .8              .8          
          CJ    0               0            
        CJSW    0               0            
        CGSO    0               0            
        CGDO    0               0            
        CGBO    0               0            
         TOX    0               0            
          XJ    0               0            
       UCRIT   10.000000E+03   10.000000E+03 
      DIOMOD    1               1            
         VFB    0               0            
        LETA    0               0            
        WETA    0               0            
          U0    0               0            
        TEMP    0               0            
         VDD    0               0            
       XPART    0               0            


**** 03/07/06 20:23:54 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Pass Transistor\Schematic1.sch


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    0.0000  (    b)    0.0000  (  Vdd)    5.0000  ($N_0001) 100.2E-09    

($N_0002)    5.0000                   ($N_0003) 100.2E-09                       

($N_0004)    5.0000                   (inv_out)    5.0000                       

(nor_out)    5.0000                   (nand_out)    5.0000                  




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -6.513E-11
    V_V2         2.004E-11
    V_V3         2.004E-11

    TOTAL POWER DISSIPATION   3.26E-10  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME            2.37
