
**** 03/07/06 20:21:40 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Ratioed Logic\Schematic1.sch


 ****     CIRCUIT DESCRIPTION


******************************************************************************




* Schematics Version 9.2
* Tue Mar 07 20:21:37 2006



** Analysis setup **
.tran 1n 2u 0 200p
.STMLIB "Schematic1.stl"


* From [PSPICE NETLIST] section of C:\Program Files\Orcad\PSpice\PSpice.ini:
.lib "nom.lib"

.INC "Schematic1.net"



**** INCLUDING Schematic1.net ****
* Schematics Netlist *



V_V1         Vdd 0 DC 5 AC 0 
V_V2         a 0   STIMULUS=V2
V_V3         b 0   STIMULUS=V3
M_M2         Vdd 0 inv_out Vdd MbreakP  
+ L=0.35u  
+ W=1u         
M_M1         inv_out a 0 0 MbreakN  
+ L=0.35u  
+ W=6u         
M_M5         Vdd 0 nand_out Vdd MbreakP  
+ L=0.35u  
+ W=1u         
M_M3         nand_out a $N_0001 0 MbreakN  
+ L=0.35u  
+ W=6u         
M_M4         $N_0001 b 0 0 MbreakN  
+ L=0.35u  
+ W=6u         
M_M9         Vdd 0 nor_out Vdd MbreakP  
+ L=0.35u  
+ W=1u         
M_M7         nor_out a 0 0 MbreakN  
+ L=0.35u  
+ W=6u         
M_M8         nor_out b 0 0 MbreakN  
+ L=0.35u  
+ W=6u         

**** RESUMING Schematic1.cir ****
.PROBE V(*) I(*) W(*) D(*) NOISE(*) 


.END

* C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Ratioed Logic\Schematic1.stl written on S
* by Stimulus Editor -- Serial Number: 1 -- Version 9.2
;!Stimulus Get
;! V2 Analog V3 Analog
;!Ok
;!Plot Axis_Settings
;!Xrange 0s 6us
;!Yrange 0 5
;!AutoUniverse
;!XminRes 1ns
;!YminRes 1n
;!Ok
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )
.STIMULUS V3 PULSE( 0 5 0 10p 10p 1u 2u )
.STIMULUS V2 PULSE( 0 5 0 10p 10p 500n 1u )

**** 03/07/06 20:21:40 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Ratioed Logic\Schematic1.sch


 ****     MOSFET MODEL PARAMETERS


******************************************************************************




               MbreakP         MbreakN         
               PMOS            NMOS            
       LEVEL    1               1            
           L  100.000000E-06  100.000000E-06 
           W  100.000000E-06  100.000000E-06 
         VTO    0               0            
          KP   20.000000E-06   20.000000E-06 
       GAMMA    0               0            
         PHI     .6              .6          
      LAMBDA    0               0            
          IS   10.000000E-15   10.000000E-15 
          JS    0               0            
          PB     .8              .8          
        PBSW     .8              .8          
          CJ    0               0            
        CJSW    0               0            
        CGSO    0               0            
        CGDO    0               0            
        CGBO    0               0            
         TOX    0               0            
          XJ    0               0            
       UCRIT   10.000000E+03   10.000000E+03 
      DIOMOD    1               1            
         VFB    0               0            
        LETA    0               0            
        WETA    0               0            
          U0    0               0            
        TEMP    0               0            
         VDD    0               0            
       XPART    0               0            


**** 03/07/06 20:21:40 ********* PSpice 9.2 (Mar 2000) ******** ID# 1 ********

 * C:\Documents and Settings\plinio\Documenti\Universit\Fondamenti di elettronica II\Schemi\Ratioed Logic\Schematic1.sch


 ****     INITIAL TRANSIENT SOLUTION       TEMPERATURE =   27.000 DEG C


******************************************************************************



 NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE     NODE   VOLTAGE


(    a)    0.0000  (    b)    0.0000  (  Vdd)    5.0000  ($N_0001)-606.3E-09    

(inv_out)    5.0000                   (nor_out)    5.0000                       

(nand_out)    5.0000                  




    VOLTAGE SOURCE CURRENTS
    NAME         CURRENT

    V_V1        -2.004E-11
    V_V2         0.000E+00
    V_V3         0.000E+00

    TOTAL POWER DISSIPATION   1.00E-10  WATTS



          JOB CONCLUDED

          TOTAL JOB TIME            1.65
